**Advanced Structures**

**Test for Consultant Inspectors**

The test will be over:

* General Provisions Sections 101-109, Removal Section 202, Concrete Sections 455, 499, Structures Sections 500-526, Material Details Sections 701, 703-712 of State of Ohio Department of Transportation’s 2013 Construction and Material Specifications
* 101,105-109, 202, 455, 499, 500-526 sections of Ohio Department of Transportation’s 2013 Construction Administration Manual of Procedures
* July 15, 2011 version of Supplemental Specification 842 Correcting Elevation of Concrete Approach Slabs with High Density Polyurethane
* December 31, 2012 version of Supplemental Specification 847 Bridge Deck Repair and Overlay with Concrete Using Scarification and Chipping
* December 31, 2012 version of Supplemental Specification 848 Bridge Deck Repair and Overlay with Concrete Using Hydrodemolition
* January 18, 2013 version of Supplemental Specification 849 Heat Straightening of Damaged Structural Steel
* Ohio Department of Transportation’s Office of Structural Engineering’s Standard Bridge Drawings Compliant with 2013 ODOT Construction and Materials Specifications