**Barrier Offset on Curved Roadways**

|  |  |  |
| --- | --- | --- |
| **Degree of Curvature**  **(Radius)** | **Required Offset** **From**  **Edge of Pavement**  **Feet** | **Minimum Width of** **Median Required**  **Feet** |
| 2.5 to 3.5 | 36 | 66 |
| 3.6 to 4.5 | 42 | 72 |
| 4.6 to 5.5 | 48 | 78 |