**Barrier Offset on Curved Roadways**

|  |  |  |
| --- | --- | --- |
| **Degree of Curvature****(Radius)** | **Required Offset** **From** **Edge of Pavement****Feet**  | **Minimum Width of** **Median Required****Feet**  |
| 2.5 to 3.5  | 36  | 66  |
| 3.6 to 4.5  | 42  | 72  |
| 4.6 to 5.5  | 48  | 78  |