**Recommended Conduit Sizes**

|  |  |
| --- | --- |
| **Usage** | **Nominal Size (ID)**  **Inches** |
| Pavement Crossovers | 3 |
| Bridge and Concrete Barrier Raceways | 2 |
| Longitudinal Conduit in Shoulder Areas | 3 |
| Structure Grounding - Embedded | 1 1/4 |
| Underpass Lighting Service | 1 1/4 |
| Conduit Ells | Same as connecting conduit,  or 2 1/2 minimum for  duct cable |
| Service Pole Pull Box to First Roadway Pull Box or Lighting Unit | 3 (minimum) |