**Types of Overhead Sign Supports**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Support Type** | **Allowable Sign Area, Sq. Ft.** | **Span or Arm Length, Ft.** | **Configuration** | **Notes** |
| TC-17.11  Span Wire | 10 to 132 | 20 to 90 |  | ----------- |
| TC-16.20  Single Arm | ------------ | Arm  23 to 45 | Diagram  Description automatically generated with medium confidence | ----------- |
| TC-12.31  Cantilever | Up to 300 (Depending on Arm Length) | Arm  26 to 30 | A picture containing transport, crane  Description automatically generated | Alternate Version - Made of Untapered Tubes. |
| TC-9.11  Semi-Overhead | Up to 150 | ------------- | Diagram, engineering drawing  Description automatically generated | Sign may be eccentric to pole. |
| TC-9.31  Center Mount | Up to 250 | \_\_\_\_\_\_\_\_\_\_ | Diagram  Description automatically generated | Sign may be  eccentric to pole. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Support Type** | **Allowable Sign Area, Sq. Ft.** | **Span or Arm Length, Ft.** | **Configuration** | **Notes** |
| TC-15.116  Steel Truss  (Steel End  Frames) | Up to 1150 | 40 to 150 | Diagram, shape, rectangle  Description automatically generated | 5' square box |
| Combination Sign  Support | According to  Sign Support | According to  Sign  Support | Diagram  Description automatically generated | May be used to add  a highway lighting  function to 16.21,  12.31, 9.11 and  9.31 |
| TC-18.24  Structure  Mounted | ----------- | ----------- | A picture containing antenna  Description automatically generated | Flush Mounting.  Aluminum Brackets |
| TC-18.26  Skewed Structure | ----------- | ----------- | A picture containing text, antenna  Description automatically generated | Aluminum Structure |