**Sign Lighting Lamps and Ballast**

|  |  |  |
| --- | --- | --- |
| **Lamp Watts** | **ANSI Lamp Code** | **Ballast Type** |
| 100  175  250 | H38HT - 100  H39KB - 175  H37KB - 250 | CMRI-100-(a)  CMRI-175-(a)  CMRI-250-(a) |

Where (a) = Operating Voltage