**Sample Phasing Chart for Actuated Signal Control**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Phase\*** | | | |
|  | **1** | **2** | **3** | **4** |
| Initial | 7 | 10 | 8 | 10 |
| Vehicle | 4 | 3 | 4 | 3 |
| Maximum | 11 | 30 | 12 | 30 |
| Yellow | 3 | 3.5 | 3 | 3.5 |
| All Red | 2 | 2 | 2 | 2 |
| Recall | ON | OFF | ON | OFF |

\* Phases as shown on **Traffic** **SCD MT-96.20** for Actuated Control.

Provide timing for the signal location under consideration.