**Decision Sight Distance for Entrance Ramp Applications**

(see Sections 607-13 and 607-15)

|  |  |  |
| --- | --- | --- |
| **Posted Mainline**  **Speed (MPH)** | **Rural**  **(Feet)** | **Urban**  **(Feet)** |
| 45 | 675 | 930 |
| 50 | 750 | 1030 |
| 55 | 865 | 1135 |
| 60 | 990 | 1280 |
| 65 | Diamond Ramp = 1050  Loop Ramp = 1220 | 1365 |
| 70 | Diamond Ramp = 1105  Loop Ramp = 1275 | 1445 |