**Codes for Use in the District System Lighting Plan**

|  |  |
| --- | --- |
|  **Code** | **Description** |
| B - | Blue | Isolated intersections which are not part of an interchange. |
| G -  | Green | Interchanges which have partial interchange lighting. |
| O - | Orange | Interchanges which have full interchange lighting. |
| P - | Pink | Roadways which are not within an interchange area, but which are between interchanges or intersections which have continuous lighting. |
| F - | Future | Unlighted locations to be lighted. |
| U - | Upgrade | Lighted locations to received more comprehensive lighting (e.g., partial interchange to full interchange). |
| D - | Downgrade | Lighted locations to be downgraded to less comprehensive lighting (e.g., full interchange to partial interchange). |
| R - | Remove | Lighted locations to become unlighted. |