**CCTV Installations (Also see TEM Section 1303-4)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Task** | **Prior Approval Needed** | **Item Description** | **Related Supplemental Specification** | **Item Master** | **Traffic SCD No.** |
| **Choose CCTV Camera** |  | CCTV IP-Camera System, Dome-Type  | 809.05.B | 809E60000 |  |
| **\*** | CCTV IP-Camera System, Type HD, Wall/Tunnel | 809.05.C | 809E60010 |  |
| **\*** | CCTV IP-Camera System, Enhanced | 809.05.E | 809E60030 |  |
| **\*** | CCTV IP-Camera System, Quad Multi-View Fixed with PTZ | 809.05.F | 809E60040 |  |
| **\*** | CCTV IP-Camera System, Multi-View | 809.05.G | 809E60050 |  |
| **\*** | CCTV IP-Camera System, Fixed View | 809.05.H | 809E60060 |  |
| If dome type camera is to be mounted on pole, choose pole height. |
| **Choose Pole Height** | \* | CCTV Concrete Pole with Lowering Unit, 50 FT | 809.06 | 809E61010 | **ITS-12.10** |
|  | CCTV Concrete Pole with Lowering Unit, 70 FT | 809.06 | 809E61000 | **ITS-12.10** |
| **Choose Cabinet Type** | \* | \*Pole Mount | 809.09.B | 809E65010 | **ITS-10.11****ITS-11.10** |
|  | Ground Mount | 809.09.A | 809E65000 | **ITS-10.10****ITS-10.11** |
| **Choose Work Pad** |  | Controller Work Pad, As Per Plan |  | 633E67200 | **ITS-10.10****ITS-10.11** |
| **Choose Grounding** |  | Ground Rod, As Per Plan |  | 625E32001 | **ITS-50.10** |
| **Choose Power Service**  |  | Underground | 809 | 625E34000 | **ITS-15.10** |
|  | Aerial | 809 | 625E34000 | **ITS-15.11** |
| **Use if directed by ODOT** | \* | ITS Cabinet-Power Distribution Cabinet (PDC) | 809.09.C | 809E65020 |  |
| \* Approval must be obtained from **Office of Traffic Operations (OTO)**  |
|