**Full-Size Walk-In Dynamic Message Sign (DMS) Installations**

**(Also see TEM Section 1303-6)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Task** | **Prior Approval Needed** | **Item Description** | **Related Supplemental Specification** | **Item Master** | **Traffic SCD No.** |
| **Choose DMS Type** | **\*** | DMS Full-Size Walk-In | 809.08.A | 809E63000 |  |
| **Choose Mount Type** |  | Overhead Sign Support, DMS Pedestal, As Per Plan |  | 630E70045 | **ITS-30.13** |
| \* | Overhead Sign Support, DMS Truss, 80’, As Per Plan |  | 630E70001 | **ITS-35.13** |
| \* | Overhead Sign Support, DMS Truss, 115’, As Per Plan |  | 630E70021 | **ITS-35.13** |
| \* | Overhead Sign Support, DMS Truss, 150’, As Per Plan |  | 630E70041 | **ITS-35.13** |
| **Choose Foundation** | **\*** | Concrete Barrier Median Overhead Sign Support Foundation, DMS Truss |  | 630E70070 | **ITS-36.12** |
|  | Overhead Sign Support Foundation, DMS Pedestal |  | 630E70082 | **ITS-30.12** |
| **\*** | Overhead Sign Support Foundation, DMS Truss |  | 630E70080 | **ITS-35.12** |
| **Choose Catwalk** | **\*** | Catwalk, DMS Truss, As Per Plan |  | 630E70051 | **ITS-35.11** |
|  | Catwalk, DMS Pedestal, As Per Plan |  | 630E70061 | **ITS-30.11** |
| **Choose Cabinet Type** | **\*** | Pole Mount | 809.09.B | 809E65010 |  |
|  | Ground Mount | 809.09.A | 809E65000 |  |
| **Choose Work Pad** |  | Controller Work Pad, As Per Plan |  | 633E67200 | **ITS-10.11** |
| **Choose Grounding** |  | Ground Rod, As Per Plan |  | 625E32001 | **ITS-50.10** |
| **Choose Power Service**  |  | Underground | 809.02 | 625E34000 | **ITS-15.10** |
|  | Aerial | 809.02 | 625E34000 | **ITS-15.11** |
| **Use if directed by ODOT** | **\*** | ITS Cabinet-Power Distribution Cabinet (PDC) | 809.09.C | 809E65020 |  |
|
| \* Approval must be obtained from **Office of Traffic Operations (OTO)** |
|